Western Australia

Building Regulations 1989

Compare between:

[01 Sep 2007, 04-f0-01] and [06 Oct 2007, 04-g0-01]

Western Australia

Local Government (Miscellaneous Provisions) Act 1960

Building Regulations 1989

## Part 1 — Preliminary

##### 1. Citation

 These regulations may be cited as the *Building Regulations 1989* 1.

##### 2. Commencement

 These regulations shall come into operation on the day that they are published in the *Government Gazette* 1.

##### 2A. Application

 (1) To the extent to which they apply to buildings that are Class 10 Buildings for the purposes of the Building Code these regulations apply in each local government district in the area specified for that district in Column 2 in Schedule 2 but not elsewhere.

 (2) Part 10 of these regulations and Part G1.1 of the Building Code apply in each local government district in the area specified for that district in Column 3 in Schedule 2 but not elsewhere.

 (3) Subject to subregulations (1) and (2) these regulations apply in each local government district in the area specified for that district in Column 4 in Schedule 2 but not elsewhere.

 [Regulation 2A inserted in Gazette 8 May 1998 p. 2369; amended in Gazette 19 Jun 1998 p. 3282.]

##### 3. Interpretation

 (1) In these regulations unless the contrary intention appears —

 **“**Act**”** means the *Local Government (Miscellaneous Provisions) Act 1960*;

 **“**approved**”** means approved by the local government except where used in relation to plans, drawings and specifications submitted for approval under section 374 of the Act, in which case **“**approved**”** has a meaning consistent with the provisions of that section;

 **“**builder**”** means a person employed to construct any building or to demolish, alter or execute any work on a building already constructed, and includes the owner or occupier of the land upon which any such building is intended to be constructed, or other person for whom, or by whose order or under whose direction and control such alteration or work was done or is intended to be done, as the case may be;

 **“**Building Code**”** means the latest edition of the Building Code of Australia published from time to time by, or on behalf of, the Australian Building Codes Board, as amended from time to time, but not including explanatory information published with that Code;

 **“**district**”** means the local government district in which a building is constructed or proposed to be constructed;

 **“**Fire Brigades Board**”** means the Western Australian Fire Brigades Board as constituted under the *Fire Brigades Act 1942*;

 **“**footing**”** means the construction by which the weight of the building is transferred to the foundations;

 **“**Form**”** means a form in Schedule 1;

 **“**local government**”** means the local government of the district in which a building is, or is proposed to be, constructed;

 **“**owner**”** includes any person in possession or receipt of the whole or any part of the rents or profits of any land or tenement or in occupation of any land or tenement otherwise than as a tenant from year to year, or for any less term, or as a tenant at will;

 **“**performance requirements**”** means the provisions of the Building Code which set out the technical requirements in accordance with which buildings must be built;

 **“**repair**”** means the reconstruction or renewal of any part of an existing building for the purpose of its maintenance but does not include alteration.

 [(2) repealed]

 (3) A reference in these regulations or in the Building Code to a code or standard shall, unless the contrary intention appears in these regulations or in the Building Code, includes a reference to that code or standard as amended from time to time.

 (4) Without derogating from section 32(1) of the *Interpretation Act 1984*, the headings of Parts, divisions and subdivisions of these regulations form part of these regulations.

 (5) Notwithstanding section 32(2) of the *Interpretation Act 1984*, the heading to a regulation in these regulations or to a portion of a regulation in these regulations forms part of these regulations.

 [Regulation 3 amended in Gazette 26 Jun 1992 p. 2758; 23 Jun 1995 p. 2442; 20 Jun 1997 p. 2821‑2 and p. 2826.]

##### 4. Exemptions

 (1) These regulations do not apply to the following buildings and work —

 (a) any building that is exempted by Statute;

 (b) temporary offices and sheds used by builders, on or about the site of any building being constructed, repaired, altered or reinstated, or used by contractors in carrying out works for any public body or corporation on or about the site of the work and used exclusively for the purpose of that building or work; but that exemption shall, however, continue only during the time occupied in completing the building or work, and in any case shall not exceed the duration of building operations, except by special permission of the local government; and

 [(c) deleted]

 (d) any building the plans, drawings and specifications of which —

 (i) were approved before these regulations came into operation in the district or in that part of the district in which the building is situated; or

 (ii) are approved pursuant to regulation 6 if that building is completed in accordance with and subject to the provisions of the by‑laws as in force before those regulations came into operation in relation to which that approval was given.

 (2) For the purposes of these regulations the re‑erection of a building that has been removed and transported from another site or from another location on the same site shall be regarded as being the erection of a new building.

 [Regulation 4 amended in Gazette 11 Jan 1991 p. 58; 20 Jun 1997 p. 2826 and 2837.]

##### 5. Building Code adopted

 (1) Subject to these regulations, the Building Code applies to and in relation to any building that can be classified according to use under Part A3 of Volume One of the Building Code and to any work referred to in Part XV of the Act and in the Building Code.

 (2) Any alteration, addition, restoration or repair to a building shall conform with these regulations but where the local government is of the opinion that any such work consists only of minor work and does not adversely affect the safety of persons accommodated in or resorting to a building or property in or in the vicinity of a building the local government may determine that the Building Code does not apply in relation to such work and that the work shall conform to only such of the provisions of the Building Code as are specified by the local government.

 [Regulation 5 amended in Gazette 11 Jan 1991 p. 58; 20 Jun 1997 p. 2822 and 2826.]

##### 6. Savings and transitional provisions

*Savings*

 (1) Where plans, drawings and specifications relating to the construction or alteration of a building on a site have been submitted to the local government for its approval and, before the local government has finally disposed of the matter —

 (a) these regulations come into operation in the district or in that part of the district in which the site is located; or

 (b) an amendment to these regulations or the Building Code comes into operation in the district or in that part of the district in which the site is located,

 the local government shall deal with the matter in accordance with the local laws, regulations and the Building Code as in operation in the district or that part of the district at the time when the plans, drawings and specifications were submitted.

*Transitional period to follow coming into operation of these regulations or amendments thereto*

 (2) Where plans, drawings and specifications relating to the construction or alteration of a building on a site are submitted to the local government for its approval then, notwithstanding that those plans, drawings and specifications do not comply with these regulations or the Building Code as in operation, at the time of their submission, in the district or in that part of the district in which the site is located, the local government may approve of those plans, drawings and specifications if the local government is satisfied that —

 (a) if those same plans, drawings and specifications had been submitted to the local government at some time during the period of 12 months prior to the date of their actual submission they would have complied with the local laws, regulations and the Building Code as in operation in the district or that part of the district; and

 (b) no undue delay has been occasioned in the submission of those plans, drawings and specifications to the local government.

 [Regulation 6 amended in Gazette 20 Jun 1997 p. 2822 and 2826; 16 Dec 2005 p. 6079.]

## Part 2 — Legal proceedings and notices

[**7.** Repealed in Gazette 20 Jun 1997 p. 2822.]

##### 8. Notices to other authorities

*Builder to give notice*

 (1) Every builder who intends to construct, alter, add to, underpin, demolish or remove any building shall, prior to the commencement of any work, give notice of that intention to any body, authority or instrumentality which is authorised under a law of the State to direct, regulate or approve the carrying out of any part of that building work.

*Powers of building surveyor*

 (2) The building surveyor may refuse to issue a building licence under the provisions of Part 4 unless or until satisfied that the provisions of subregulation (1) have been complied with, and that the approval of such of the authorities therein mentioned as may apply to the particular case has been obtained, or may issue a building licence or demolition licence subject to compliance with the requirements of those authorities.

 (3) Notwithstanding the provisions of subregulation (2) the building surveyor shall before issuing a building licence liaise with the Fire Brigades Board for the purposes of the fire prevention and public safety requirements of the Building Code.

 (4) Subregulation (3) does not apply to Class 1 and Class 10 Buildings of the Building Code.

[Part 3 (r. 9) repealed in Gazette 20 Jun 1997 p. 2822.]

## Part 4 — Building applications

##### 10. Application for licence

 (1) Every builder intending to construct a building or alter, add to, repair or underpin, demolish or remove an existing building shall before commencing —

 (a) that construction, alteration, addition, repair or underpinning, demolition or removal; or

 (b) any earthworks necessary for, or incidental to, that construction, alteration, addition, repair or underpinning, demolition or removal,

 make written application to the local government for a licence to commence that work.

*Form and lodging of application*

 (2) Applications made under subregulation (1) shall be in the form of Form 2 or 3, whichever is appropriate, and shall be lodged at the office of the building surveyor.

 [Regulation 10 amended in Gazette 20 Jun 1997 p. 2826.]

##### 11. Particulars to accompany application

*Builder to submit drawings etc.*

 (1) Every builder making application for a building licence shall deposit with the building surveyor —

*Building details*

 (a) 2 complete sets of drawings (to scale not less that 1:100) showing —

 (i) a plan of every storey;

 (ii) at least 2 elevations of external fronts;

 (iii) one or more sections, transverse or longitudinal;

 (iv) the heights of each storey;

 (v) depth of foundations;

 (vi) underpinnings;

 (vii) levels of ground;

 (viii) construction of the walls, floors and roofs; and

 (ix) any other information that the building surveyor may require, all clearly figured and dimensioned;

*Block details*

 (b) a block and drainage plan (to a scale not less than 1:500) showing —

 (i) street names, lot number, and title reference to the site with the north point clearly marked;

 (ii) the size and shape of the site;

 (iii) the dimensioned position of proposed new building and of any existing buildings on the site;

 (iv) the relative levels of the site with respect to the street or way adjoining;

 (v) the position and size of any existing sewers and existing stormwater drains;

 (vi) the position of street trees, if any, between the site and the roadway;

*Specifications*

 (c) 2 copies of specifications describing materials to be used in the construction and, where not indicated on the drawings, the sizes thereof together with all other information not shown on the drawings, which is necessary to show that the building will, if constructed in accordance with the specifications, comply with the provisions of the Building Code;

*Performance levels and requirements*

 (d) when required by the building surveyor —

 (i) a list of the performance requirements applicable to that building which will be satisfied by a method other than that set out in the Deemed‑to‑Satisfy Provisions of the Building Code;

 (ii) details of assessment methods to be used to establish compliance with those listed requirements;

 (iii) details of any expert certificates relied on to establish compliance with those listed requirements, including the extent of the reliance and the qualifications of the expert;

 (iv) details of any tests or calculations used to establish compliance with those listed requirements; and

 (v) details of any standards or other documents relied on to establish compliance with those listed requirements;

 (da) any other details required by the building surveyor to establish compliance with the Building Code; and

*Cost estimate*

 (e) the estimated value (calculated in the manner set out in regulation 24(2)) of the proposed construction and, when so required by the building surveyor, the name and address of any registered architect, practising structural engineer or other person under whose supervision the construction is to be carried out.

*CodeMark certificates*

 (1a) For the purposes of the application, a CodeMark certificate issued for a building product is sufficient evidence that the building product complies with the provisions of the Building Code specified in the certificate.

 (1b) In subregulation (1a) —

 **“**building product**”** includes a building product, method, design, component and system;

 **“**CodeMark certificate**”** means a certificate, issued under the CodeMark Scheme administered by the Australian Building Codes Board, which certifies that a building product, method, design, component or system complies with the specified provisions of the Building Code.

*Compliance with fire requirements*

 (2) Notwithstanding the provision of subregulation (1) every builder making application for a building licence, excluding Classes 1 and 10 of the Building Code, shall deposit with the Fire Brigades Board plans and specifications of sufficient detail to enable the Fire Brigades Board to assess their compliance with the Fire Requirements of the Building Code of Australia.

*Requirements as to drawings*

 (3) The drawings referred to in subregulation (1) shall be legible and durable and shall be not less in size than sheet A4.

*New and existing work*

 (4) All new work shall be clearly delineated on the drawings as distinct from existing work by colouring or other suitable means.

*Particulars to accompany application for demolition licence*

 (5) An application for a licence to demolish or remove a building shall be accompanied by particulars of the location of the building, and such other particulars as the local government may require.

*Particulars of levels to be supplied where earthworks involved*

 (6) Without limiting the generality of subregulation (1)(a)(vii) where any alteration is proposed to the existing conformation of the ground on the site involving earthworks of any description the local government may require the drawings referred to in that paragraph to show all levels, both new and old, clearly marked or indicated by contour lines or in such other manner as the local government may direct.

 [Regulation 11 amended in Gazette 23 Jun 1995 p. 2442‑3; 20 Jun 1997 p. 2823 and 2826; 16 Dec 2005 p. 6079.]

##### 12. Copies for records

*Copies to be retained*

 (1) One copy of every drawing, plan, specification or calculation shall remain in the office of the building surveyor as a permanent record.

*Plans etc. may be inspected by or with consent of owner*

 (2) The owner or mortgagee of any building or any person authorised in writing by the owner or mortgagee may, during the normal office hours of the local government, inspect any plan or other document relating to that building retained pursuant to subregulation (1).

*Inspection by police officer*

 (3) This regulation does not prevent a police officer from being permitted to inspect a plan or other document in the course of duty in connection with a situation in which the safety of a person is at risk.

 [Regulation 12 amended in Gazette 26 Jun 1992 p. 2758; 20 Jun 1997 p. 2826.]

##### 13. Commencement of work

*Buildings or alterations*

 (1) A builder shall not commence to construct, alter, add to or underpin any building and shall not commence any earthworks, necessary for, or incidental to, that construction, alteration, addition or underpinning until —

 (a) the plans, drawings and specifications have been approved;

 (b) the building surveyor has stamped the plans, drawings and specifications with the official stamp showing the number of the approval and the date of approval;

 (c) the builder has paid the appropriate fee prescribed in the Table to regulation 24; and

 (d) a licence has been issued in the form of Form 4 or 5.

*Demolition*

 (2) A builder shall not commence to demolish or remove any building until —

 (a) he has paid the appropriate fee prescribed in the Table to regulation 24; and

 (b) a licence has been issued in the form of Form 7.

##### 14. Examination of drawings etc.

*Building surveyor to examine*

 (1) The building surveyor shall examine all plans, drawings, and specifications deposited with him or her, but if any such plans, drawings or specifications are, in the building surveyor’s opinion not in conformity with the requirements of this Part or not clear or not easily legible, or do not contain sufficient information, he or she may, within 15 days of their deposit with him or her, return them to the builder for amendment, and in that case the plans, drawings and specifications shall be considered as not having been deposited with the building surveyor until re‑submitted by the builder.

*Disapproval of drawings etc.*

 (2) If —

 (a) the local government; or

 (b) the building surveyor, acting pursuant to a delegation under section 374(1b) of the Act,

 refuses to approve any plan, drawing or specification, notice of the refusal to approve shall be given in writing to the builder and the reasons for the refusal to approve shall be stated in the notice, together with details of the builder’s rights under Part XV of the Act to apply to the State Administrative Tribunal for a review of the refusal.

 [Regulation 14 amended in Gazette 20 Jun 1997 p. 2823 and 2826; 30 Dec 2004 p. 6949.]

##### 15. Duration of licence

*Building licence*

 (1) A building licence in the form of Form 4 is void if the work covered by the licence (the building) is not substantially commenced within 12 months of the date of the issue of the licence; but at any time after the expiry of 12 months the approval of the local government or the building surveyor, as the case may be, to the plans, drawings and specifications previously approved may, if those plans, drawings and specifications are still in conformity with these regulations, be again obtained subject to the payment of any further fees and the lodging of such further plans, drawings and specifications as the local government or building surveyor may at its or his or her discretion require.

*Demolition licence*

 (2) A demolition licence in the form of Form 7 is void if the work covered by the licence is not commenced within 12 months of the date of the issue of the licence.

 [Regulation 15 amended in Gazette 20 Jun 1997 p. 2826.]

##### 16. Building left incomplete

*Time for completion*

 (1) Where a licence is issued under these regulations for the construction of a building that building shall be completed within 24 months of the date of the issue of the licence, or such other time as approved by local government.

*Consequences of failure to complete*

 (2) Where work on the construction of a building is commenced but is not completed within the time prescribed by subregulation (1) the provisions of section 409A of the Act apply.

 [Regulation 16 amended in Gazette 20 Jun 1997 p. 2826.]

##### 17. Departure from approved plans

 No variation from or alteration of approved plans, drawings and specifications shall be made by any builder without the consent of the building surveyor in writing having been first obtained, and any alteration or departure from the approved plans, drawings and specifications shall, on the consent of the building surveyor therefor being notified, be drawn, described, and endorsed on and in the plans, drawings and specifications.

##### 18. Preliminary plans and provisional approvals

*Plans may be lodged with owner’s consent*

 (1) Notwithstanding anything contained in this Part any person having paid the fees prescribed in item 2 of the Table to regulation 24 may submit to the building surveyor preliminary plans, drawings and specifications of any building proposed to be constructed, accompanied by the written consent of the owner of the site of the proposed building to the lodging of those plans, drawings and specifications for examination and report as to whether such proposal is capable of being executed in conformity with these regulations.

*Application for provisional approval*

 (2) Without limiting the operation of subregulation (1) a person may apply to the local government for its provisional approval of a proposed building, by lodging with the application —

 (a) the fee prescribed in item 2 of the Table to regulation 24;

 (b) preliminary plans, elevations and sections of the proposed buildings; and

 (c) such concise specifications or descriptions as the local government may require to satisfy itself as to the nature of the building and its intended use.

*Consideration by local government*

 (3) The local government may after considering the report of the building surveyor on an application made pursuant to subregulation (2) give its provisional approval for the construction of the proposed building, if, when constructed, it would conform to these regulations as in force, at the time of the making of the application, in the district or in that part of the district in which the building is proposed to be constructed.

*Duration of provisional approval*

 (4) A provisional approval given pursuant to subregulation (3) shall remain in force for a period of 12 months from the date on which it is given.

*Effect of provisional approval*

 (5) A provisional approval given pursuant to subregulation (3) has the effect, notwithstanding any provision of these regulations to the contrary, of enabling the person to whom it is given, during the period that it is in force, to procure the issue of a licence for the commencement of work on the proposed building, if the final plans, drawings and specifications are in conformity with the provisional approval and the fees prescribed in the Table to regulation 24 are paid.

 [Regulation 18 amended in Gazette 12 Jul 1991 p. 3458; 20 Jun 1997 p. 2823 and 2826.]

## Part 5 — Certificate of classification

##### 19. Classification of buildings

 Every building shall be classified by the local government in accordance with Part A3 of Volume One of the Building Code.

 [Regulation 19 inserted in Gazette 20 Jun 1997 p. 2823.]

##### 20. Certificate of classification

*Preparation*

 (1) Where approval is given for the erection of a building the local government shall —

 (a) on completion of the building; or

 (b) where it consents in writing to the occupation of portion of the building concerned before the completion of the entire building concerned,

 prepare a certificate of classification, in duplicate, in the form, or to the effect, of Form 1.

*Issue*

 (2) The original of the certificate shall be issued to the person on whose behalf the building was erected.

*Inspection of certificates*

 (3) The duplicate shall be retained in the local government’s office and shall be open to inspection free of charge by any person during the normal office hours of the local government.

*No occupation until certificate is issued*

 (4) A person shall not occupy any portion of a building until a certificate of classification has been issued in accordance with these regulations.

*Non‑application to Class 1 or Class 10 building*

 (5) This regulation does not apply to a Class 1 or 10 building of the Building Code.

 [Regulation 20 amended in Gazette 20 Jun 1997 p. 2824 and 2826.]

##### 21. Certificate for a building occupied in stages

 Where a certificate of classification has been issued for portion of an uncompleted building and the local government approves the occupation of a further portion of the building, it shall —

 (a) revoke that certificate; and

 (b) issue a further certificate of classification in accordance with regulation 20 covering all portions of the building for which approval to occupy has been given by the local government.

 [Regulation 21 amended in Gazette 20 Jun 1997 p. 2826.]

##### 22. Change of use

*Application of regulation*

 (1) This regulation applies to any building, whether erected before or after the commencement of these regulations.

 (2) The use of a building shall not be changed from that of one Class to that of another Class unless —

 (a) the building complies with the requirements of the Building Code applicable to the new Class; and

 (b) the change of use has been approved by the local government.

*Change of use to be notified*

 (3) Before making any change in the use of a building which would result in a change of classification under these regulations, the person proposing to make that change shall notify the local government in writing, setting out the nature of the proposed change of use.

*New certificate*

 (4) Upon approving a change of use the local government shall —

 (a) revoke any certificate of classification already in existence for the building; and

 (b) prepare a certificate of classification in accordance with regulation 20 in respect of the new use; and

 (c) issue the original of that certificate to the person proposing the change of use.

 [Regulation 22 amended in Gazette 20 Jun 1997 p. 2826.]

##### 23. Offences

 A person who uses or occupies or permits the use or occupation of a building in contravention of regulation 20(4) or 22 is guilty of an offence.

 Penalty: $5 000 and in addition a daily penalty of $100 for each day during which the offence continues.

 [Regulation 23 amended in Gazette 20 Jun 1997 p. 2824.]

## Part 6 — Fees

##### 24. Scale of fees

 (1) The scale of fees set out in the Table to this regulation shall be chargeable by and received by a local government on an application for any licence, or for services to be rendered or provided under these regulations.

 (2) For the purposes of item 1 of the Table to this regulation —

 (a) where the construction work is to be carried out under a contract, the estimated value of the construction work shall be the contract price, where that price includes value for at least each of the components referred to in paragraph (b); and

 (b) where the construction work is carried out other than under a contract or under a contract the contract price for which does not include value for each of the following components, the estimated value of the construction work shall be the sum of the value of all goods (including manufactured goods) forming part of the construction work, labour, services necessary, fees payable, overheads to be met and profit margin.

**Table
Scale of fees**

| **Item Description** | **Fee** |
| --- | --- |
| 1. Building licence —  |  |
|  (a) For the issue of a building licence for a new building of Class 1 or 10 or for alterations or additions to an existing building of Class 1 or 10. | 0.35% of  of the estimated value of the proposed construction as determined by the local government, but not less than $40. |
|  (b) For the issue of a building licence for a new building of a Class other than Class 1 or 10 or for alterations or additions to an existing building of a Class other than Class 1 or 10. | 0.2% of  of the estimated value of the proposed construction as determined by the local government, but not less than $40. |
| 2. Preliminary plans |  |
|  For the examination of, and a report on, preliminary plans. | 25% of the fee for the issue of a building licence to carry out the proposed construction described in the plans. |
| 3. Materials on, or excavation of, a street For the issue of a licence for the deposit of materials on, or the excavation of, a street. | $1 per month or part of a month for each m2 of the area of the street enclosed by any hoarding or fence. |
| 4. Demolition |  |
|  For the issue of a licence to demolish a building. | $50 for each storey. |

 [Regulation 24 amended in Gazette 12 Jul 1991 p. 3457‑8; erratum in Gazette 19 Jul 1991 p. 3625; amended in Gazette 23 Jun 1995 p. 2443; 20 Jun 1997 p. 2824 and 2826; 28 Jul 2000 p. 4014.]

## Part 7 — Precautions during construction

##### 25. Licences under section 377 of the Act

 A licence issued under section 377 of the Act shall be in the form of Form 6.

##### 26. Hoardings

*General*

 (1) The erection, maintenance, lighting and removal of hoardings and fences shall be carried out in accordance with the provisions of Part XV of the Act and with such other requirements as the building surveyor may specify in order to ensure the safety and convenience of the public.

*Limit of encroachment*

 (2) A hoarding or fence erected pursuant to Part XV of the Act, or under a licence issued under section 377 of the Act shall not encroach at pavement level past half the width of the public footway or such other width as determined by the local government.

 [Regulation 26 amended in Gazette 20 Jun 1997 p. 2826.]

##### 27. Protection of adjacent property

*Shoring and underpinning*

 (1) Where an excavation or demolition is to be made in proximity to an existing building that building shall be protected to ensure stability.

*Additional precautions*

 (2) Where the foundation of an existing building is of material likely to become unstable as a result of the excavation of adjoining ground, additional precautions, to the satisfaction of the building surveyor shall be taken to ensure its stability.

*Building work affecting building of adjoining owner*

 (3) The provisions of section 391 of the Act apply in relation to building work described in subsection (1) of that section.

*Damage by vibration*

 (4) Where any building operations or earthworks involve the use of equipment that may, in the opinion of the local government, cause damage by vibration to the property of an owner of land in the vicinity of the land on which such operations or earthworks are carried out, the local government may impose requirements as to the manner of carrying out such operations or earthworks for the purpose of minimising such damage, and effect shall be given thereto.

 [Regulation 27 amended in Gazette 20 Jun 1997 p. 2826.]

##### 28. Protection of excavation

 Every excavation for a building shall be properly guarded and protected and shall, where necessary, be sheet piled so as to prevent caving in of the adjoining earth or pavement, and in any case required by the building surveyor, sheet piling of an approved type shall be utilized to protect the subsoil from damage by scour of subsoil or surface waters.

##### 29. Storage of material on streets etc.

*Permissible in certain circumstances only*

 (1) A builder shall not deposit or store any material on a street, way, or other public place except for the purpose of immediate transportation of that material onto the building site or ground being used for the purposes of building operations, and the deposit and transportation shall be carried out as expeditiously as possible, and at such times, as in special circumstances the building surveyor may direct, so as to cause the least possible obstruction to traffic on the street or way, and with due precautions for the public safety and convenience.

*No restriction where licence has been obtained*

 (2) Any part of the street or way for which the builder has procured a licence for use and enclosure by a hoarding, shall be deemed part of the building site for the purposes of this Part for the period covered by that licence.

## Part 8 — Precautions during demolition

##### 30. Licence to take down buildings

 A licence issued under section 374A of the Act shall be in the form of Form 7.

##### 31. Demolition of buildings

 (1) Any person demolishing or removing any building or part of a building shall ensure that —

 (a) before any demolition work commences —

 (i) notification shall be given to —

 (A) Telstra (within the meaning given in the *Telstra Corporation Act 1991* (Commonwealth) section 3) and arrangements made for disconnection of its services; and

 (B) the relevant electricity corporation, Gas Corporation or other supply authority and arrangements shall be made for the disconnection of energy services to the building, or the part of the building to be demolished; and

 (C) Water Corporation (established by the *Water Corporation Act 1995* section 4) and arrangements made for disconnection of its services;

 and

 (ii) a certificate shall be obtained from the Health Surveyor of the local government certifying that the building to be demolished has been treated so as to ensure that it is not infested by rodents;

 (b) where the building to be demolished comprises more than 1 storey, the demolition shall be effected by the complete removal of 1 storey after another, commencing with the uppermost storey and proceeding with the successive removal of the storeys in descending order, or other method approved by the local government;

 (c) no part of an external wall abutting on a street or road shall be demolished, except during such hours as are permitted by the building surveyor;

 (d) unless otherwise authorised by the building surveyor, any material removed or displaced from the building shall not be placed upon a floor of the building but shall be immediately lowered to the ground and thereafter removed from the site, but in no case shall loading be such as to cause a floor to collapse;

 (e) materials removed or displaced from the building shall not be placed in any street, road or right of way and, before commencing work, as the case may require, shall be kept sprayed with water so as to prevent any nuisance from dust;

 (f) materials removed or displaced from the building being demolished or materials left standing shall not be burned on the demolition site;

 (g) the local government shall be notified of the existence of any septic tank(s) on the demolition site 7 days prior to the emptying and filling of such tank(s);

 (h) any septic tank(s) on the demolition site shall be emptied and filled with clean sand or removed entirely and any soakwells, leach drains or similar apparatus shall be removed or filled with clean sand;

 (i) where the building being demolished is more than 1 storey in height, a hoarding and an overhead gantry shall be provided to protect pedestrians;

 (j) where required by the local government, a footpath deposit shall be lodged with the local government to cover the cost of any damage caused to footpaths during the demolition operation, against which the actual cost of repairing any damage will be charged and any unexpended balance refunded to the person taking out the licence. In the event of the cost of repairs being in excess of the deposit lodged, the person holding the licence shall, on demand, pay the amount of the excess to the local government;

 (k) where necessary, the holder of a licence shall construct a temporary crossing place over the footpath as specified by the local government;

 (l) the demolition site shall be cleared, and left clean and tidy to the satisfaction of the building surveyor within 90 days of the date of commencement of the demolition or such other time as agreed by the local government;

 (m) the fee for this licence has been paid being the fee set out in item 4 of the Table to regulation 24; and

 (n) the provisions of the *Occupational Safety and Health Regulations 1996* are complied with in relation to the demolition work.

 (2) In subregulation (1)(a)(i)(B) —

 **“**relevant electricity corporation**”** means the Electricity Networks Corporation, the Electricity Retail Corporation or the Regional Power Corporation, established by section 4 of the *Electricity Corporations Act 2005*, as the case requires.

 [Regulation 31 amended in Gazette 11 Jan 1991 p. 58; 12 Jul 1991 p. 3458; 20 Jun 1997 p. 2824‑5 and 2826; 31 Mar 2006 p. 1342; 5 Oct 2007 p. 5327-8.]

## Part 9 — Projection beyond street alignments

##### 32. Construction of projections

*Footings*

 A footing shall not project beyond the street alignment except that where the top of the footing —

 (a) is more than 750 mm and less than 3 m below the pavement level, the footing may extend 300 mm beyond the street alignment; and

 (b) is 3 m or more below the pavement level, the footing may extend 750 mm beyond the street alignment.

##### 33. Minimum height above pavement

 A projection shall not extend beyond the street alignment at any height less than 2 750 mm from the level of the public footway but the provisions of this regulation do not apply to —

 (a) footings constructed in accordance with the provisions of regulation 32; or

 (b) mouldings which do not project more than 12 mm beyond the street alignment in any portion of a shop front.

 [Regulation 33 amended in Gazette 20 Jun 1997 p. 2825.]

[**34.** Repealed in Gazette 12 Nov 1993 p. 6151.]

##### 35. Windows, balconies etc.

 A balcony shall not encroach over a street, way or public place to a greater distance than that provided by section 400(2) of the Act, and a balcony or window shall not project more than 900 mm beyond the street alignment in a street over 12 m in width, or more than 600 mm in a street from 10 m to 12 m in width, and —

 (a) any part of a projection where it overhangs a street shall be not less than 2 750 mm above the level of the street and be not nearer than 1 200 mm to the centre of the nearest party wall or to any adjoining building or allotment not in the same occupation;

 (b) the aggregate length of any projections shall not exceed one‑half of the length of the wall of the building on the level of the floor on which the projections are made;

 (c) a projecting window shall not exceed a total overall width of 3 600 mm and the distance between any 2 projecting windows shall not be less than one‑half of the aggregate width of those windows;

 (d) projecting windows shall not be connected by a balcony having any portion projecting beyond the street alignment.

 [Regulation 35 amended in Gazette 20 Jun 1997 p. 2825.]

##### 36. Gates, doors etc., abutting on street

 A person shall not construct or hang any gate, door, window, or shutter in such a manner that any part of the gate, door, window or shutter when being opened projects over any street or way at a height less than 2 750 mm above the level of the pavement.

 [Regulation 36 amended in Gazette 20 Jun 1997 p. 2825; 28 Jul 2000 p. 4014.]

##### 37. Window shutters

 Notwithstanding the provisions of this Part, window shutters are permitted if they project not more than 50 mm beyond the street alignment when in the fully open position.

## Part 10 — Private swimming pools

 [Heading inserted in Gazette 26 Jun 1992 p. 2758.]

##### 38. Certain provisions of the Building Code not to apply

 The following provisions of the Building Code do not apply —

 (a) in Volume One —

 (i) Objective G01(c);

 (ii) Functional Statement GF1.2; and

 (iii) Performance Requirement GP1.2;

 and

 (b) in Volume Two —

 (i) Objective O2.5(b);

 (ii) Functional Statement F2.5.2; and

 (iii) Performance Requirement P2.5.3.

 [Regulation 38 inserted in Gazette 20 Jun 1997 p. 2825.]

##### 38A. Definitions

 In this Part —

 **“**access through a building**”** means access between the area within an enclosure and a part of a building to which there is direct or indirect access from outside the enclosure;

 **“**Australian Standard AS 1926.1**”** means Australian Standard AS 1926.1 — 1993 incorporating Amendment No. 1 only;

 **“**swimming pool**”** means a swimming pool, within the meaning of section 245A(1) of the Act, in which there is water that is more than 300 mm deep;

 **“**young child**”** means a child under the age of 5 years.

 [Regulation 38A inserted in Gazette 26 Jun 1992 p. 2758; amended in Gazette 12 Nov 1993 p. 6151; 20 Jun 1997 p. 2826; 19 Oct 2001 p. 5610; 14 Dec 2001 p. 6399; 4 May 2007 p. 1965.]

##### 38B. Enclosure of pool

 (1) Except as provided in subregulation (2) and regulation 38D(2), the owner or occupier of premises on which there is a swimming pool is to install or provide around the pool an enclosure suitable to restrict access by young children to it and its immediate surrounds.

 Penalty: $5 000 and a daily penalty of $250.

 (2) If the pool is at the rear of the premises, a person does not contravene subregulation (1) only because the area enclosed includes, as well as the pool and its immediate surrounds, any other part of the rear portion of the premises.

 (3) Despite subregulation (2), an enclosure is not suitable for the purposes of subregulation (1) if a building other than a Class 10a building under the Building Code is included within the area enclosed unless all external doors and windows in that building satisfy the requirements of Australian Standard AS 1926.1, but a Class 10a building may be included within the area enclosed even though any external door or window in it does not satisfy those requirements.

 (4) Except as provided by this Part, the enclosure is not suitable for the purposes of subregulation (1) unless —

 (a) it consists of a fence, wall, gate or other barrier, or a combination of them;

 (b) any fence, wall, gate or other barrier included in the enclosure is in accordance with the requirements of Australian Standard AS 1926.1 or alternative requirements that the local government approves; and

 (c) any wall that it includes contains no means of access through a building other than —

 (i) a window that is in accordance with the requirements of Australian Standard AS 1926.1; or

 (ii) a door that is approved by the local government under regulation 38C.

 (5) The local government is not to approve alternative requirements under subregulation (4)(b) unless it is satisfied that the requirements will restrict access by young children to the swimming pool as effectively as Australian Standard AS 1926.1.

 (6) If a boundary fence of the premises is a part of the enclosure of a pool, the boundary fence satisfies the requirements of clauses 2.3, 2.6 and 2.7 of Australian Standard AS 1926.1 if all those requirements are satisfied in relation to either side of the fence.

 [Regulation 38B inserted in Gazette 14 Dec 2001 p. 6400; amended in Gazette 5 Apr 2002 p. 1827; 4 May 2007 p. 1965.]

##### 38C. Approval of doors by local government

 (1) The local government may approve a door for the purposes of regulation 38B(4)(c)(ii) if the door is in accordance with the requirements of Australian Standard AS 1926.l and —

 (a) in the opinion of the local government, to install between the building and the pool a fence or barrier satisfying regulation 38B would involve —

 (i) a sufficient problem of a structural nature; or

 (ii) a sufficient problem of any other nature, the cause of which is neither within the control of the owner nor occupier;

 (b) the pool is totally enclosed by a building; or

 (c) in the opinion of the local government, the existence between the building and the pool of a fence or barrier satisfying regulation 38B would create a sufficient problem for a person with a disability who is resident at the premises and wishes to have access to the pool.

 (2) In deciding whether to give approval under subregulation (1) a local government is to place particular weight on whether or not a young child resides at the premises.

 (3) In this regulation —

 **“**person with a disability**”** means a person who is able to produce a certificate given by ACROD Limited (Western Australian Division) (ACN 008445485), registered under the *Corporations Act 2001* of the Commonwealth, certifying that the person has a disability that makes it difficult for the person to use a gate of the kind that would be required by these regulations in a swimming pool fence.

 [Regulation 38C inserted in Gazette 14 Dec 2001 p. 6401.]

##### 38D. Concessions for pre‑November 2001 pools

 (1) This regulation applies to a swimming pool —

 (a) installed before 5 November 2001; or

 (b) installed on or after 5 November 2001 in accordance with plans, drawings and specifications submitted to the local government for approval before that day.

 (2) Even though the pool is not one to which regulation 38B(2) applies, a person does not contravene regulation 38B(1) only because the area enclosed includes, as well as the pool and its immediate surrounds, any other part of the premises.

 (3) The enclosure required by regulation 38B(1) may include a wall that contains a door permitting access through a building if that door satisfies the requirements of Australian Standard AS 1926.l.

 [Regulation 38D inserted in Gazette 14 Dec 2001 p. 6401‑2.]

[**38E.** Repealed in Gazette 12 Nov 1993 p. 6153.]

##### 38F. Maximum inspection charge

 For the purposes of section 245A(8)(b) of the Act, the maximum charge is $55.

 [Regulation 38F inserted in Gazette 26 Jun 1992 p. 2760; amended in Gazette 28 Jul 2000 p. 4014.]

##### 38G. Transitional

 Regulation 6(2) does not apply in relation to the requirements of this Part.

 [Regulation 38G inserted in Gazette 26 Jun 1992 p. 2760.]

##### 38H. Infringement notices

 (1) The offence of failing to enclose a swimming pool as required by regulation 38B(1) is prescribed for the purposes of section 9.16(1) of the Act.

 (2) The modified penalty that is to be specified in an infringement notice given for that offence is —

 (a) if a notice under section 245A(5)(b) of the Act has been served, $200;

 (b) if a notice under section 245A(5)(b) of the Act has not been served, $100.

 [Regulation 38H inserted in Gazette 24 Jun 1996 p. 2863; amended in Gazette 20 Jun 1997 p. 2825; 14 Dec 2001 p. 6402.]

## Part 10A — Hot water systems and water use

 [Heading inserted in Gazette 21 Aug 2007 p. 4174.]

##### 38I. Hot water systems and water use: Building Code amended

 (1) The Building Code Volume Two Appendix A Contents on page 621 is amended by deleting the box and the words in it and adding instead —

“

 **WESTERN AUSTRALIA**

 **Application of Western Australian additions**

 **WA 1 — Hot Water Systems**

 **WA 1.1 Performance Provision**

 **WA 1.1.0 Performance requirement**

 **WA 1.2 Deemed‑to‑Satisfy Provision**

 **WA 1.2.0 Hot water system standard**

 **WA 1.3 Acceptable Construction Practice**

 **WA 2 — Water Use**

 **WA 2.1 Definitions**

 **WA 2.1.0 Definitions**

 **WA 2.2 Performance Provisions**

 **WA 2.3 Performance Requirement**

 **WA 2.3.0 Water use efficiency**

 **WA 2.3.1 Water loss prevention**

 **WA 2.3.2 Hot water use efficiency**

 **WA 2.4 Deemed‑to‑Satisfy Provision**

 **WA 2.4.0 Water use efficiency**

 **WA 2.4.1 Swimming pool covers and blankets**

 **WA 2.4.2 Hot water use efficiency**

 **WA 2.5 Acceptable Construction Practice**

 ”.

 (2) The Building Code Volume Two Appendix A Western Australia Additions (page 623) is amended by deleting “Western Australia has no additions to the Housing Provisions.” and adding instead —

“

 **Application of Western Australian additions**

 This Appendix contains additional provisions for application in Western Australia as follows:

|  |
| --- |
| WA 1 — HOT WATER SYSTEMS |

 **WA 1.1 PERFORMANCE PROVISION**

 **WA 1.1.0 Performance requirement**

 A building’s hot water system including any associated components must produce low levels of greenhouse gases when heating water.

 **WA 1.2 DEEMED‑TO‑SATISFY PROVISION**

 **WA 1.2.0 Hot water system standard**

 A hot water system must be one of the following —

 (a) a solar hot water system that —

 (i) complies with AS 2712‑2002; and

 (ii) has been tested in accordance with AS 4234‑1994; and

 (iii) achieves a minimum energy saving of 60% for a hot water demand level of 38 MJ per day for climate zone 3;

 (b) a gas hot water system that —

 (i) complies with AS 4552‑2005; and

 (ii) achieves a minimum energy rating of 5 stars in accordance with AS 4552‑2005;

 (c) a heat pump hot water system that —

 (i) complies with AS 2712‑2002; and

 (ii) has been tested in accordance with AS 4234‑1994; and

 (iii) achieves a minimum energy saving of 60% for a hot water demand level of 38 MJ per day for climate zone 3.

 **WA 1.3 ACCEPTABLE CONSTRUCTION PRACTICE**

 Compliance with Deemed‑to‑Satisfy provision of WA 1.2.0 satisfies the Performance Requirement WA 1.1.0 for a building.

|  |
| --- |
| WA 2 — WATER USE |

 **WA 2.1 DEFINITIONS**

 **WA 2.1.0 Definitions**

 The following definitions are used in this part —

 potable water means water intended for human consumption supplied by the holder of an operating licence within the meaning given in the *Water Services Licensing Act 1995* section 3.

 WELS has the meaning given in the *Water Efficiency Labelling and Standards Act 2005* of the Commonwealth section 7.

 **WA 2.2 PERFORMANCE PROVISIONS**

 **Objective**

 The objective of these provisions is to reduce water demand by —

 (a) using water efficiently; and

 (b) minimising water wastage.

 **Functional statement**

 To reduce potable water demand a building is to be capable of —

 (a) using potable water efficiently; and

 (b) preventing excessive loss of potable water.

 **WA 2.3 PERFORMANCE REQUIREMENT**

 **WA 2.3.0 Water use efficiency**

 A building must have features that, to the degree necessary, facilitate the efficient use of potable water appropriate to —

 (a) the geographic location of the building; and

 (b) the available potable water supply for the building; and

 (c) the function and use of the building.

 **WA 2.3.1 Water loss prevention**

 A building, including any water holding structure, must have features that, to the degree necessary, prevent the excessive loss of potable water appropriate to —

 (a) the geographic location of the building; and

 (b) the available potable water supply for the building; and

 (c) the function and use of the building; and

 (d) the effects of permanent features such as topography, structures and buildings.

 **WA 2.3.2 Hot water use efficiency**

 A building must have features that, to the degree necessary, facilitate the efficient use of hot water appropriate to —

 (a) the geographic location of the building; and

 (b) the available hot water supply for the building; and

 (c) the function and use of the building.

 **WA 2.4 DEEMED‑TO‑SATISFY PROVISION**

 **WA 2.4.0 Water use efficiency**

 (a) All tap fittings other than bath outlets and garden taps must be a minimum of 4 stars WELS rated.

 (b) All shower heads must be a minimum of 3 stars WELS rated.

 (c) All sanitary flushing systems must be a minimum of 4 stars WELS rated dual flush.

 **WA 2.4.1 Swimming pool covers and blankets**

 An outdoor private swimming pool or spa associated with a Class 1 building must be supplied with a cover, blanket or the like that —

 (a) is designed to reduce water evaporation; and

 (b) is accredited with the Smart Approved Watermark under the Smart Approved Watermark Scheme governed by the Australian Water Association, the Irrigation Association of Australia, the Nursery and Garden Industry Australia and the Water Services Association of Australia.

 **WA 2.4.2 Hot water use efficiency**

 All internal hot water outlets (such as taps, showers and washing machine water supply fittings) must be connected to a hot water system or a recirculating hot water system with pipes installed and insulated in accordance with AS/NZS 3500:2003: Plumbing and Drainage, Part 4 Heated Water Services.

 The pipe from the hot water system or recirculating hot water system to the furthest hot water outlet must not exceed 20 metres in length or 2 litres of internal volume.

 **WA 2.5 ACCEPTABLE CONSTRUCTION PRACTICE**

 Compliance with all of the Deemed‑to‑Satisfy provisions of WA 2.4.0 satisfies the Performance Requirement WA 2.3.0 for a building.

 Compliance with all of the Deemed‑to‑Satisfy provisions of WA 2.4.1 satisfies the Performance Requirement WA 2.3.1 for a building.

 Compliance with all of the Deemed‑to‑Satisfy provisions of WA 2.4.2 satisfies the Performance Requirement WA 2.3.2 for a building.

”.

 [Regulation 38I inserted in Gazette 21 Aug 2007 p. 4174‑8.]

## Part 11 — Miscellaneous

##### 39. Loading notice plates to be posted on completion of certain buildings

 (1) On completion of any Class 5, 6, 7 or 8 building and before occupation of any such building, any floor or part of a floor which has been designed to sustain a uniformly distributed live load exceeding 5kPa shall have a notice conspicuously and permanently posted adjacent thereto in the form hereunder indicating the actual loadings for which the floor or part of the floor has been structurally designed.

|  |
| --- |
| Designed Floor Loading Distributed kg/m2 Concentrated kg |

*Design and position of notice plates*

 (2) The lettering of a notice posted pursuant to subregulation (1) shall be embossed or cast into a metal tablet not less than 230 mm square and located not less than 1 m above floor level.

[**40.** Repealed in Gazette 11 Nov 1994 p. 5707.]

[**41.** Repealed in Gazette 20 Jun 1997 p. 2825.]

##### 42. Offences and penalties

*Offences*

 (1) Where, by these regulations anything is directed, or forbidden, to be done, or authority is given to any person to direct, or forbid, anything to be done and that authority is exercised, any person failing or neglecting to do anything so directed, or doing anything so forbidden, commits an offence.

*Penalties*

 (2) A person who commits an offence against these regulations is liable to the penalty expressly mentioned in relation to the offence, or, if no penalty is expressly mentioned, to a penalty not exceeding $5 000.

 [Regulation 42 amended in Gazette 20 Jun 1997 p. 2825.]

[**43.** Omitted under the Reprints Act 1984 s. 7(4)(f).]

Schedule 1 — Forms

**Form 1. Certificate of classification**

|  |
| --- |
| *Local Government (Miscellaneous Provisions) Act 1960*, s. 374C*Building Regulations 1989*, reg 20(1)**CERTIFICATE OF BUILDING****CLASSIFICATION** |

|  |
| --- |
| **Local Government**: |

|  |  |  |  |
| --- | --- | --- | --- |
| **Building** | Address | No.: | Street name: |
| Suburb: | Postcode: |
| Lot/location No.: |

|  |  |  |
| --- | --- | --- |
| **Classification** |  Storey or portion of building |  Classification(s) |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

|  |  |
| --- | --- |
| **Chief****Executive****Officer** | Name: |
| Signature: | Date: |

[Form 1 inserted in Gazette 20 Jun 1997 p. 2826.]

**Form 2. Application for building licence**

|  |  |
| --- | --- |
| *Local Government (Miscellaneous Provisions) Act 1960*,s. 374*Building Regulations 1989*, reg. 10(2)**Building licence application** |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Property where** **building to be built** | Street | No.: | Street name: |
| address | Suburb: | Postcode: |
| Lot/location No.: | Is lot free of improvements?: yes/no |
|  |
| **Property owner(s) (attach separate page if more than 2)** | Name: | Phone: |
| Address: |
| Name: | Phone: |
| Address: |
|  |
| **Details of work (tick box or boxes)** | Type of building to be constructed:🞏 Single dwelling 🞏 Patio 🞏 Swimming pool 🞏 Warehouse🞏 Grouped dwelling 🞏 Outbuilding 🞏 Retaining wall 🞏 Office🞏 Pergola 🞏 Factory 🞏 Shop🞏 Other (specify): |
| Estimated floor area of building (m2): |
| Estimated value of construction work (including the GST): $ |
|  |
| **Applicant (if applicant is not builder)** | Name: |
| Address: |
|  | Postal address: |
|  | Phone (H): (W): (Mob): |
|  | Fax: Email: |
|  | Signature: | Date: |
|  |
|  |
| **Applicant (if applicant is builder or owner builder)** | Name: |
| Address: |
| Postal address: |
|  | Phone (H): (W): (Mob): |
|  | Fax: Email: |
|  | Applicant’s registration number under the *Builders’ Registration Act 1939*: |
|  | Contact name: |
|  | Signature: | Date: |

[Form 2 inserted in Gazette 30 Sep 2003 p. 4257‑8.]

**Form 3. Application for demolition licence**

|  |  |
| --- | --- |
| *Local Government (Miscellaneous Provisions) Act 1960*, s. 374A*Building Regulations 1989*, reg. 10(2)**APPLICATION FOR DEMOLITION LICENCE** | (Office use)Application no.:\_\_\_\_\_\_\_\_\_\_ |

|  |
| --- |
| **Local Government:** |
|  |
| **Building to be demolished** | Address | No.: | Street name: |
|  | Suburb: | Postcode: |
| Lot/location No.: |
| Certificate of Title | Volume:  | Folio: |
| To be demolished: 🞏 Whole of building 🞏 Part only of building. Give details: |
| Type of construction (e.g. brick & tile): |
| Number of storeys: |
| Previous use or classification: |
|  |
| **Owner** | Name: |
| Address: |
|  |
| **Demolition contractor** | Name: |
| Address: |
| Phone number: Fax number: |
|  |
| **Applicant** | Name: |
| Address: |
| Phone numbers (H): (W): |
| Fax number: Email: |
| Signature: | Date: |

[Form 3 inserted in Gazette 20 Jun 1997 p. 2828.]

**Form 4. Building licence**

|  |  |
| --- | --- |
| *Local Government (Miscellaneous Provisions) Act 1960*, s. 374*Building Regulations 1989*, reg.13(1)(d)**BUILDING LICENCE** | Licence no.:\_\_\_\_\_\_\_\_\_\_\_\_ |

|  |
| --- |
| **Local Government:** |
|  |
| **Licensee** | Name: |
| Address: |
|  |
| **Property where building to be built** | Address | No.: | Street name: |
| Suburb: | Postcode: |
| Lot/location No.: |
| Certificate of Title | Volume:  | Folio: |
|  |
| **Details of work** | 🞏 New building  Type of building (e.g.: residential, shop, factory, warehouse): |
| 🞏 Alteration or addition to existing building Type of alteration or addition (e.g.: carport, bedroom, second storey, store room, office, toilet, games room): |
| The building work permitted by this licence — • must be carried out in accordance with the plans, drawings and specifications submitted with Application for Building Licence no. ; and• must be carried out in accordance with the conditions set out on the back of this licence.If the building work permitted by this licence is not substantially commenced within 12 months of the date of this licence, the licence will become void.The building has been assessed as being of Class(es)  |
|  |
| **Building surveyor** | Name: |
| Signature: | Date: |

**Note:** The licensee must produce this licence and the approved plans, drawings and specifications whenever requested by the building surveyor.

**Back of Form 4**

**CONDITIONS**

|  |
| --- |
| This licence is subject to the following conditions.If you are dissatisfied with these conditions you may apply to the State Administrative Tribunal for a review under section 374 of *Local Government (Miscellaneous Provisions) Act 1960*. |

[Form 4 inserted in Gazette 20 Jun 1997 p. 2829-30; amended in Gazette 30 Dec 2004 p. 6949.]

**Form 5. Special building licence**

|  |  |
| --- | --- |
| *Local Government (Miscellaneous Provisions) Act 1960*, s. 399(4)*Building Regulations 1989*, reg*.* 13(1)(d)**SPECIAL BUILDING LICENCE** | Licence no.:\_\_\_\_\_\_\_\_\_\_\_\_ |

|  |
| --- |
| **Local Government:** |
|  |
| **Licensee** | Name: |
| Address: |
|  |
| **Property where building to be built** | Address | No.: | Street name: |
| Suburb: | Postcode: |
| Lot/location No.: |
| Certificate of Title | Volume:  | Folio: |
|  |
| **Details of work** | 🞏 New building  Type of building (e.g.: residence, shop, factory, warehouse): |
| 🞏 Alteration or addition to existing building Type of alteration or addition (e.g.: carport, bedroom, second storey, store room, office, toilet, games room): |
| 🞏 Temporary building  Type of building (e.g.: marquee, grandstand, stage): |
| The building work permitted by this licence must be carried out in accordance with — • the plans, drawings and specifications submitted with Application for Building Licence no. ; and• the conditions set out on the back of this licence.The building has been assessed as being of Class(es)  |
|  |
| **Building surveyor** | Name: |
| Signature: | Date: |

**Note:** The licensee must produce this licence and the approved plans, drawings and specifications whenever requested by the building surveyor.

**Back of Form 5**

**CONDITIONS**

|  |
| --- |
| This licence is subject to the following conditions.If you are dissatisfied with these conditions you may apply to the State Administrative Tribunal for a review under section 399 of *Local Government (Miscellaneous Provisions) Act 1960*. |

[Form 5 inserted in Gazette 20 Jun 1997 p. 2831-2; amended in Gazette 30 Dec 2004 p. 6949.]

**Form 6. Licence to deposit building material on, or excavate near, a street**

|  |  |
| --- | --- |
| *Local Government (Miscellaneous Provisions) Act 1960*, s. 377*Building Regulations 1989*, reg. 25**LICENCE TO DEPOSIT BUILDING MATERIAL ON, OR EXCAVATE NEAR, A STREET** | Licence no.:\_\_\_\_\_\_\_\_\_\_\_\_ |

|  |
| --- |
| **Local Government:** |
|  |  |
| **Licensee** | Name: |
| Address: |
|  |  |
| **Property where building to be built or excavation to be carried out** | Address | No.: | Street name: |
| Suburb: | Postcode: |
| Lot/location No.: |
| Certificate of Title | Volume:  | Folio: |
|  |  |  |  |
| **Details of deposit or excavation** | 🞏 Deposit of building material on a street Type of material: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Name of street: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_m Part of street (e.g.: outside No. 10): \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| 🞏 Excavation near a street Reason for excavation: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Name of street: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Part of street likely to be affected (e.g.: outside No. 10): \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| Period during which part of street may be enclosed: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ to \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |
| Maximum area of the street which may be enclosed: Frontage: \_\_\_\_\_\_\_\_\_\_\_\_ m Width: \_\_\_\_\_\_\_\_\_\_\_\_ m Height: \_\_\_\_\_\_\_\_\_\_\_\_ m. |
| The deposit of building material or excavation permitted by this licence must be carried out in accordance with the conditions set out on the back of this licence. |
|  |
| **Deposit** | The local government acknowledges receipt of a deposit of $ \_\_\_\_\_\_\_\_\_\_ paid by the licensee under section 377(4) of the Act. |
|  |
| **Building surveyor** | Name: |
| Signature: | Date: |

**Back of Form 6**

**CONDITIONS**

|  |
| --- |
| This licence is subject to the following conditions.1. Every excavation must be securely fenced off from the street to the satisfaction of the building surveyor.2. When building materials are deposited on a street the licensee must install and maintain —  (a) hoardings around the deposited material;  (b) gangways to allow vehicular and pedestrian access along the street; and (c) water channels to allow water to drain from the area, which are constructed from materials, and to a design, approved by the building surveyor.3. The licensee must ensure that the area around any excavation or deposited material is sufficiently lit during darkness to ensure the safety of persons using the street. 4. On or before the last day on which this licence permits the licensee to enclose part of the street, the licensee must —  • remove all hoardings, gangways, channelling, building material and debris from the street; and • repair, to the satisfaction of the building surveyor, any damage caused to the street (including the road surface, kerbing and footpaths). If you are dissatisfied with these conditions you may, within 14 days of the granting of this licence, apply to the State Administrative Tribunal for a review under section 377 of the *Local Government (Miscellaneous Provisions) Act 1960*. |

[Form 6 inserted in Gazette 20 Jun 1997 p. 2833-4; amended in Gazette 30 Dec 2004 p. 6950.]

**Form 7. Demolition licence**

|  |  |
| --- | --- |
| *Local Government (Miscellaneous Provisions) Act 1960*, s. 374A*Building Regulations 1989*, regs. 13(2) and 30**DEMOLITION LICENCE** | Licence no.:\_\_\_\_\_\_\_\_\_\_ |
|  |
| **Local Government:** |
|  |
| **Licensee** | Name: |
| Address: |
|  |  |
| **Demolition contractor:** |
|  |
| **Building to be demolished** | Address | No.: | Street name: |
| Suburb: | Postcode: |
| Lot/location No.: |
| Certificate of Title | Volume: | Folio: |
| To be demolished: 🞏 Whole of building 🞏 Part only of building. Details: |
| Type of construction (e.g. brick & tile): |
| Number of storeys: |
| Previous use or classification: |
| The demolition work permitted by this licence must be — • carried out in accordance with the details set out in Application for Demolition Licence no. ; • carried out in accordance with the conditions set out on the back of this licence; and• commenced within 12 months of the date of this licence. |
|  |
| **Building surveyor** | Name: |
| Signature: | Date: |

**Back of Form 7**

**CONDITIONS**

|  |
| --- |
| This licence is subject to the following conditions.If you are dissatisfied with these conditions you may be able to apply to the State Administrative Tribunal for a review under section 374A of *Local Government (Miscellaneous Provisions) Act 1960*. |

[Form 7 inserted in Gazette 20 Jun 1997 p. 2835-6; amended in Gazette 30 Dec 2004 p. 6950.]

Schedule 2 — Application

[r. 2A]

| **Column 1** | **Column 2** | **Column 3** | **Column 4** |
| --- | --- | --- | --- |
| **District** | **Class 10 Buildings** | **Part 10**  | **Rest of regulations** |
| Albany | Whole district | Whole district | Whole district |
| Armadale | Whole district | Whole district  | Whole district |
| Augusta‑Margaret River | Whole district | Whole district | Whole district |
| Bassendean | Whole district | Whole district | Whole district |
| Bayswater | Whole district | Whole district | Whole district |
| Belmont | Whole district | Whole district | Whole district |
| Beverley | Whole district | Whole district | Whole district |
| Bridgetown‑Greenbushes | Whole district | Whole district | Whole district |
| Brookton | Whole district | Whole district | Whole district |
| Broome | Whole district | All townsites | Whole district |
| Broomehill | All townsites and area described in Note 1 | All townsites | Whole district |
| Bruce Rock | All townsites | All townsites | Whole district |
| Bunbury | Whole district | Whole district | Whole district |
| Busselton | Whole district  | Whole district | Whole district |
| Cambridge | Whole district | Whole district | Whole district |
| Canning | Whole district | Whole district | Whole district |
| Capel | Whole district | Whole district | Whole district |
| Carnamah | All townsites | All townsites | Whole district |
| Carnarvon | Whole district except Gascoyne‑Minilya Ward  | Whole district | Whole district |
| Claremont | Whole district | Whole district | Whole district |
| Cockburn | Whole district | Whole district | Whole district |
| Collie | Whole district | Whole district | Whole district |
| Coorow | All townsites | Whole district | Whole district |
| Corrigin | Townsite of Corrigin | All townsites | Whole district |
| Cottesloe | Whole district | Whole district | Whole district |
| Cranbrook | All townsites | All townsites | Whole district |
| Cuballing | Whole district | All townsites | Whole district |
| Cue | All townsites | All townsites | Whole district |
| Cunderdin | All townsites | All townsites | Whole district |
| Dalwallinu | All townsites | All townsites | Whole district |
| Dandaragan | All townsites | All townsites | Whole district |
| Dardanup | Whole district | Whole district | Whole district |
| Denmark | Whole district | All townsites | Whole district |
| Derby‑West Kimberley | All townsites | Whole district | Whole district |
| Dowerin | All townsites | All townsites | Whole district |
| Dumbleyung | Townsites of Dumbleyung, Kukerin | Whole district | Whole district |
| East Fremantle | Whole district | Whole district | Whole district |
| Esperance | All townsites | All townsites | Whole district |
| Fremantle | Whole district | Whole district | Whole district |
| Geraldton | Whole district | Whole district | Whole district |
| Gnowangerup | All townsites | All townsites | Whole district |
| Gosnells | Whole district | Whole district | Whole district |
| Greenough | Whole district | Whole district | Whole district |
| Hall’s Creek | Whole district | All townsites and area subject to Halls Creek Town Planning Scheme | Whole district |
| Harvey | Whole district | All townsites and area zoned Special Residential or Special Rural by Shire of Harvey Town Planning Scheme | Whole district |
| Jerramungup | Whole district except areas zoned rural by a town planning scheme | Whole district except areas zoned rural by a town planning scheme | Whole district |
| Joondalup | Whole district | Whole district | Whole district |
| Kalamunda | Whole district | Whole district | Whole district |
| Kalgoorlie‑Boulder | Whole district | Whole district | Whole district |
| Katanning | Whole district | Whole district | Whole district |
| Kellerberrin | Townsites of Kellerberrin, Doodlakine and Baandee | Townsites of Kellerberrin, Doodlakine and Baandee | Whole district |
| Kent | Townsites of Nyabing, Pingrup | Townsites of Nyabing, Pingrup | Townsites of Nyabing, Pingrup |
| Kojonup | All townsites | All townsites | Whole district |
| Koorda | All townsites and Avon location 16386 | Whole district | Whole district |
| Kwinana | Whole district | Whole district | Whole district |
| Lake Grace | All townsites | All townsites | Whole district |
| Laverton | All townsites | All townsites | All townsites |
| Leonora | All townsites | All townsites | Whole district |
| Mandurah | Whole district | Whole district | Whole district |
| Manjimup | Whole district | Whole district | Whole district |
| Meekatharra | All townsites | All townsites | All townsites |
| Melville | Whole district | Whole district | Whole district |
| Menzies | All townsites | All townsites | All townsites |
| Merredin | Townsites of Burracoppin, Hines Hill, Korbel, Merredin, Muntadgin, Nangeenan, Nokaning, Nukarni | Townsites of Burracoppin, Hines Hill, Korbel, Merredin, Muntadgin, Nangeenan, Nokaning, Nukarni | Whole district |
| Mingenew | All townsites | Whole district | Whole district |
| Moora | All townsites | All townsites | Whole district |
| Morawa | All townsites | All townsites | Whole district |
| Mosman Park | Whole district | Whole district | Whole district |
| Mt Marshall | All townsites | All townsites | Whole district |
| Mt Magnet | All townsites | All townsites | All townsites |
| Mukinbudin | All townsites | All townsites | Whole district |
| Mullewa | All townsites | All townsites | Whole district |
| Mundaring | Whole district | Whole district | Whole district |
| Murchison | None | None | None |
| Murray | Whole district except areas zoned rural by local laws or a town planning scheme | Whole district | Whole district |
| Narembeen | All townsites | All townsites | Whole district |
| Narrogin (Shire) | Whole district except areas zoned for farming purposes by a town planning scheme | All townsites | Whole district |
| Narrogin (Town) | Whole district | Whole district | Whole District |
| Nedlands | Whole district | Whole district | Whole district |
| Northam (Town) | Whole district | Whole district | Whole district |
| Northam (Shire) | Whole district | Whole district | Whole district |
| Northampton | Whole district | Whole district | Whole district |
| Nungarin | All townsites | All townsites | Whole district |
| Peppermint Grove | Whole district | Whole district | Whole district |
| Perenjori | All townsites and areas subject to town planning schemes | All townsites | Whole district |
| Perth | Whole district | Whole district | Whole district |
| Plantagenet | Whole district | Whole district | Whole district |
| Port Hedland | All townsites | All townsites | Whole district |
| Quairading | All townsites | Whole district | Whole district |
| Ravensthorpe | Whole district except areas zoned general agricultural by a town planning scheme | Whole district except areas zoned general agricultural by a town planning scheme | Whole district |
| Rockingham | Whole district | Whole district | Whole district |
| Sandstone | All townsites in Sandstone Ward | Sandstone Ward | Sandstone Ward |
| Serpentine‑Jarrahdale | Whole district | Whole district | Whole district |
| South Perth | Whole district | Whole district | Whole district |
| Stirling | Whole district | Whole district | Whole district |
| Subiaco | Whole district | Whole district | Whole district |
| Swan | Whole district | Whole district | Whole district |
| Tammin | Townsite of Tammin | Townsite of Tammin | Townsite of Tammin |
| Three Springs | All townsites | All townsites | Whole district |
| Trayning | Townsites of Trayning, Kununoppin, Yelbeni | Townsites of Trayning, Kununoppin, Yelbeni | Townsites of Trayning, Kununoppin, Yelbeni |
| Victoria Park | Whole district | Whole district | Whole district |
| Victoria Plains | Whole district | All townsites | Whole district |
| Vincent | Whole district | Whole district | Whole district |
| Wagin | All townsites in Town Ward or Williams loc. 440, 507, 545, 618, 945, 1165 or 5330 | Whole district | Whole district |
| Wandering | Townsite of Wandering and areas zoned rural residential by local laws or a town planning scheme | Whole district | Whole district |
| Wanneroo | Whole district | Whole district | Whole district |
| Waroona | Whole district | Whole district | Whole district |
| West Arthur | All townsites | All townsites | Whole district |
| Wickepin | All townsites | All townsites | Whole district |
| Williams | All townsites | All townsites | Whole district |
| Wiluna | Townsite of Wiluna | Townsite of Wiluna | Townsite of Wiluna |
| Wongan‑Ballidu | Townsites of Wongan Hills, Ballidu, Cadoux, Kondut, Burakin | Townsites of Wongan Hills, Ballidu, Cadoux, Kondut, Burakin | Townsites of Wongan Hills, Ballidu, Cadoux, Kondut, Burakin |
| Woodanilling | Townsite of Woodanilling | Whole district | Whole district |
| Wyalkatchem | Whole district | Whole district | Whole district |
| Wyndham‑EastKimberley | Whole district | Whole district | Whole district |
| Yalgoo | All townsites | All townsites | Whole district |
| Yilgarn | All townsites | All townsites | All townsites |
| York | Whole district | Whole district | Whole district |
| All other districts  | Whole district | All townsites | Whole district |

**Note 1 — Broomehill**

(a) Broomehill Suburban Lots 362, 363, 372 to 423, 427 to 432, 438, 445, 446, 603 to 605, 609 and 610.

(b) Lot 17 to 24 being portion of Kojonup Location 256.

(c) Kojonup Location 1671.

(d) Reserves 8163, 10285, 10431 and 17230.

 [Schedule 2 inserted in Gazette 5 Apr 2002 p. 1827‑32; amended in Gazette 4 Apr 2003 p. 1026‑7; 13 Aug 2004 p. 3251; 18 May 2007 p. 2257.]

Notes

1 This is a compilation of the *Building Regulations 1989* and includes the amendments made by the other written laws referred to in the following table. The table also contains information about any reprint.

Compilation table

| **Citation** | **Gazettal** | **Commencement** |
| --- | --- | --- |
| *Building Regulations 1989* | 28 Jul 1989 p. 2261‑93 | 28 Jul 1989 (see r. 2) |
| *Building Amendment Regulations 1991* | 11 Jan 1991 p. 58‑9 | 11 Jan 1991 |
| *Building Amendment Regulations (No. 2) 1991* | 12 Apr 1991 p. 1638 | 12 Apr 1991 (see r. 2) |
| *Building Amendment Regulations (No. 3) 1991* | 31 May 1991 p. 2682‑3 | 31 May 1991 |
| *Building Amendment Regulations (No. 4) 1991* | 12 Jul 1991 p. 3457‑8(erratum 19 Jul 1991 p. 3625) | 1 Aug 1991 (see r. 2) |
| *Building Amendment Regulations 1992* | 26 Jun 1992 p. 2757‑60 | 1 Jul 1992 (see r. 2) |
| *Building Amendment Regulations 1993* | 12 Nov 1993 p. 6151‑3 | 12 Nov 1993 |
| *Building Amendment Regulations 1994* | 11 Nov 1994 p. 5706‑7 | 11 Nov 1994 |
| *Building Amendment Regulations 1995* | 23 Jun 1995 p. 2442‑3 | 23 Jun 1995 |
| **Reprint of the *Building Regulations 1989* as at 22 Nov 1995** (includes amendments listed above) |
| *Building Amendment Regulations 1996* | 24 Jun 1996 p. 2863 | 1 Jul 1996 (see r. 2) |
| *Building Amendment Regulations 1997* | 20 Jun 1997 p. 2821‑36 | 1 Jul 1997 (see r. 2) |
| *Building Amendment Regulations (No. 2) 1997* | 20 Jun 1997 p. 2837 | 1 Jul 1997 (see r. 2) |
| **Reprint of the *Building Regulations 1989* as at 18 Jul 1997** (includes amendments listed above) |
| *Building Amendment Regulations 1998* | 8 May 1998 p. 2369‑73 | 8 May 1998 |
| *Building Amendment Regulations (No. 2) 1998* | 19 Jun 1998 p. 3282‑6 | 19 Jun 1998 |
| *Building Amendment Regulations 1999* | 12 Feb 1999 p. 479‑85 | 12 Feb 1999 |
| *Building Amendment Regulations (No. 2) 1999* | 24 Sep 1999 p. 4666‑7 | 24 Sep 1999 |
| *Building Amendment Regulations 2000* | 28 Jul 2000 p. 4013‑14 | 28 Jul 2000 |
| **Reprint of the *Building Regulations 1989* as at 2 Mar 2001** (includes amendments listed above) |
| *Building Amendment Regulations 2001* | 19 Oct 2001 p. 5609‑12 | 5 Nov 2001 (see r. 2) |
| *Building Amendment Regulations (No. 2) 2001*3 | 14 Dec 2001 p. 6399‑402 | 18 Mar 2002 (see r. 2) |
| *Building Amendment Regulations 2002*4 | 5 Apr 2002 p. 1826‑32 | 5 Apr 2002 |
| *Building Amendment Regulations 2003* | 4 Apr 2003 p. 1026‑7 | 4 Apr 2003 |
| *Building Amendment Regulations (No. 2) 2003* | 30 Sep 2003 p. 4256‑8 | 30 Sep 2003  |
| *Building Amendment Regulations 2004* | 13 Aug 2004 p. 3250‑1 | 13 Aug 2004 |
| *Building Amendment Regulations (No. 2) 2004* | 30 Dec 2004 p. 6949‑50 | 1 Jan 2005 (see r. 2 and *Gazette* 31 Dec 2004 p. 7130) |
| **Reprint 4: The *Building Regulations 1989* as at 11 Mar 2005** (includes amendments listed above) |
| *Building Amendment Regulations 2005* | 16 Dec 2005 p. 6078-9 | 16 Dec 2005 |
| *Electricity Corporations (Consequential Amendments) Regulations 2006* r. 68 | 31 Mar 2006 p. 1299‑57 | 1 Apr 2006 (see r. 2) |
| *Building Amendment Regulations 2007* | 4 May 2007 p. 1964-5 | 4 May 2007 |
| *Building Amendment Regulations (No. 2) 2007* | 18 May 2007 p. 2256-7 | 18 May 2007 |
| *Building Amendment Regulations (No. 3) 2007* | 21 Aug 2007 p. 4174-8 | r. 1 and 2: 21 Aug 2007 (see r. 2(a));Regulations other than r. 1 and 2: 1 Sep 2007 (see r. 2(b)) |
| *Building Amendment Regulations (No. 4) 2007* | 5 Oct 2007 p. 5327-8 | r. 1 and 2: 5 Oct 2007 (see r. 2(a));Regulations other than r. 1 and 2: 6 Oct 2007 (see r. 2(b)) |

2 Repealed on 1 July 1999 by No. 59 of 1997 s. 3 (Cwlth). Now see the *Telecommunications Act 1997* (Cwlth).

3 The *Building Amendment Regulations (No. 2) 2001* r. 7 reads as follows:

“

7. Transitional

 (1) In this regulation —

 **“access through a building not of Class 10a”** means access between the area within an enclosure and a part of a building, other than a Class 10a building under the Building Code, to which there is direct or indirect access from outside the enclosure;

 **“pre‑July 1992 pool”** means a swimming pool that —

 (a) was installed before 1 July 1992; or

 (b) was installed on or after 1 July 1992 in accordance with plans, drawings and specifications that were submitted to the local government for approval before that day;

 **“transitional period”** means the period beginning on the day on which these regulations come into operation and —

 (a) unless paragraph (b) applies, ending on 17 December 2006; or

 (b) if the swimming pool is on premises sold within the period referred to in paragraph (a), ending on the day 3 months after the settlement day for that sale.

 (2) During the transitional period an enclosure for a pre‑July 1992 pool may, for the purposes of regulation 38B(1) of the *Building Regulations 1989*, include a wall containing a door or window permitting access through a building not of Class 10a even though —

 (a) the door or window may not satisfy the requirements of Australian Standard AS 1926.1; and

 (b) the door may not have been approved by the local government.

 (3) If a swimming pool was installed before 28 July 1989, during the transitional period a gate in its enclosure may open in any direction.

”.

4 The *Building Amendment Regulations 2002* r. 5 reads as follows:

“

5. Transitional

 (1) In this regulation —

 **“pre‑July 1992 pool”** means a swimming pool that —

 (a) was installed before 1 July 1992; or

 (b) was installed on or after 1 July 1992 in accordance with plans, drawings and specifications that were submitted to the local government for approval before that day;

 **“transitional period”** means the period beginning on the day on which these regulations come into operation and —

 (a) unless paragraph (b) applies, ending on 17 December 2006; or

 (b) if the swimming pool is on premises sold within the period referred to in paragraph (a), ending on the day 3 months after the settlement day for that sale.

 (2) During the transitional period, despite regulation 38B(3) of the *Building Regulations 1989* a building may be included within the area enclosed for a pre‑July 1992 pool even though —

 (a) the building is not a Class 10a building under the Building Code; and

 (b) any external door or window in the building does not satisfy the requirements of Australian Standard AS 1926.1.

”.