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Work Health and Safety Legislation (Workplace Exposure Limits) Amendment Regulations 2026
Made by the Governor in Executive Council.
[bookmark: _Toc244776066][bookmark: _Toc244776311][bookmark: _Toc244776625][bookmark: _Toc244776712]Part 1 — Preliminary
[bookmark: _Toc244776067][bookmark: _Toc244776713]1.	Citation
[bookmark: Start_Cursor]		These regulations are the Work Health and Safety Legislation (Workplace Exposure Limits) Amendment Regulations 2026.
[bookmark: _Toc244776068][bookmark: _Toc244776714]2.	Commencement
		These regulations come into operation as follows —
	(a)	Part 1 — on the day on which these regulations are published on the WA legislation website;
	(b)	the rest of the regulations — on 1 December 2026.
[bookmark: _Toc244776069][bookmark: _Toc244776314][bookmark: _Toc244776628][bookmark: _Toc244776715]Part 2 — Work Health and Safety (General) Regulations 2022 amended
[bookmark: _Toc244776070][bookmark: _Toc244776716]3.	Regulations amended
		This Part amends the Work Health and Safety (General) Regulations 2022.
[bookmark: _Toc244776071][bookmark: _Toc244776717]4.	Regulation 5 amended
	(1)	In regulation 5 delete the definition of exposure standard.
	(2)	In regulation 5 insert in alphabetical order:

	exposure limit means an exposure limit in the Workplace exposure limits for airborne contaminants as modified by regulation 48A;
	mg/m3 means milligrams per cubic metre of air;
	ppm means parts of a contaminant per million parts of air;
	Workplace exposure limits for airborne contaminants means the document of that name published by Safe Work Australia dated November 2025;

[bookmark: _Toc244776072][bookmark: _Toc244776718]5.	Regulation 33 amended
		In regulation 33 in example 1 delete “standard.” and insert:

		limit.

[bookmark: _Toc244776073][bookmark: _Toc244776719]6.	Regulation 48A inserted
		At the beginning of Chapter 3 Part 3.2 Division 7 insert:

[bookmark: _Toc244776074][bookmark: _Toc244776720]48A.	Modifications to exposure limits
	(1)	This regulation modifies the text of the Workplace exposure limits for airborne contaminants.
	(2)	The Table in Appendix A is modified by deleting the row relating to Diesel particulate matter (as respirable elemental carbon).
	(3)	The Table in Appendix A is modified in the row relating to Phosphine by deleting the 8‑hour time weighted averages (TWA) of 0.05 ppm and 0.07 mg/m3 and the peak limits of 0.15 ppm and 0.21 mg/m3 and inserting the following exposure limits — 
	(a)	8‑hour time weighted average (TWA) — 
	(i)	0.3 ppm; and
	(ii)	0.42 mg/m3;
	(b)	short term exposure limit (STEL) — 
	(i)	1 ppm; and
	(ii)	1.4 mg/m3.
	(4)	In subregulation (3), each of the following terms has the same meaning as in the Workplace exposure limits for airborne contaminants — 
	8‑hour time weighted average (TWA)
	peak limitation (peak limit)
	short term exposure limit (STEL)
	(5)	The modification in subregulation (3) applies until 30 November 2029.

[bookmark: _Toc244776075][bookmark: _Toc244776721]7.	Regulation 49 amended
	(1)	In regulation 49(1) delete “standard” and insert:

		limit

	(2)	In regulation 49(2):
	(a)	delete “standard” and insert:

		limit

	(b)	delete “time‑weighted” and insert:

		time weighted

	(c)	in paragraph (a) delete “mg per cubic metre of air;” and insert:

		mg/m3;

	(d)	in paragraph (b) delete “mg per cubic metre of air.” and insert:

		mg/m3.

	(3)	In regulation 49(3):
	(a)	delete “Workplace Exposure Standards for Airborne Contaminants” and insert:

		Workplace exposure limits for airborne contaminants

	(b)	delete “standard referred to in those Standards.” and insert:

		limit referred to in that document.

	(4)	Delete regulation 49(4) and insert:

	(4)	In subregulation (2), each of the following terms has the same meaning as in the Workplace exposure limits for airborne contaminants — 
	8‑hour time weighted average
	inhalable
	respirable

	Note: The heading to amended regulation 49 is to read:
		Ensuring exposure limits for substances and mixtures not exceeded
[bookmark: _Toc244776076][bookmark: _Toc244776722]8.	Regulation 50 amended
		In regulation 50(1):
	(a)	delete “standard” (1st occurrence) and insert:

		limit

	(b)	in paragraph (a) delete “standard; or” and insert:

		limit; or

[bookmark: _Toc244776077][bookmark: _Toc244776723]9.	Regulation 352 amended
		In regulation 352(c) delete “standard;” and insert:

		limit;

[bookmark: _Toc244776078][bookmark: _Toc244776724]10.	Regulation 420 amended
		In regulation 420(2) delete “standard” and insert:

		limit

[bookmark: _Toc244776079][bookmark: _Toc244776725]11.	Regulation 454 amended
		In regulation 454(2)(a) delete “to below the exposure standard; and” and insert:

		below the exposure limit for asbestos; and

[bookmark: _Toc244776080][bookmark: _Toc244776726]12.	Regulation 455 amended
		In regulation 455(2) delete “to below the exposure standard.” and insert:

		below the exposure limit for asbestos.

[bookmark: _Toc244776081][bookmark: _Toc244776727]13.	Regulation 482 amended
		In regulation 482(1) and (2) delete “standard” and insert:

		limit for asbestos

[bookmark: _Toc244776082][bookmark: _Toc244776728]14.	Regulation 529CA amended
		In regulation 529CA(2)(e) delete “workplace exposure standard;” and insert:

		exposure limit for respirable crystalline silica;

[bookmark: _Toc244776083][bookmark: _Toc244776729]15.	Regulation 529CE amended
		In regulation 529CE(b) delete “workplace exposure standard” and insert:

		exposure limit for respirable crystalline silica

[bookmark: _Toc244776084][bookmark: _Toc244776730]16.	Schedule 8 amended
		In Schedule 8 clause 3(2)(a)(iv) delete “standard” and insert:

		limit

[bookmark: _Toc244776085][bookmark: _Toc244776330][bookmark: _Toc244776644][bookmark: _Toc244776731]Part 3 — Work Health and Safety (Mines) Regulations 2022 amended
[bookmark: _Toc244776086][bookmark: _Toc244776732]17.	Regulations amended
		This Part amends the Work Health and Safety (Mines) Regulations 2022.
[bookmark: _Toc244776087][bookmark: _Toc244776733]18.	Regulation 5 amended
	(1)	In regulation 5 delete the definition of exposure standard.
	(2)	In regulation 5 insert in alphabetical order:

	exposure limit means an exposure limit in the Workplace exposure limits for airborne contaminants as modified by regulation 48A;
	mg/m3 means milligrams per cubic metre of air;
	ppm means parts of a contaminant per million parts of air;
	Workplace exposure limits for airborne contaminants means the document of that name published by Safe Work Australia dated November 2025;

[bookmark: _Toc244776088][bookmark: _Toc244776734]19.	Regulation 33 amended
		In regulation 33 in example 1 delete “standard.” and insert:

		limit.

[bookmark: _Toc244776089][bookmark: _Toc244776735]20.	Regulation 48A inserted
		At the beginning of Chapter 3 Part 3.2 Division 7 insert:

[bookmark: _Toc244776090][bookmark: _Toc244776736]48A.	Modifications to exposure limits
	(1)	This regulation modifies the text of the Workplace exposure limits for airborne contaminants.
	(2)	The Table in Appendix A is modified in the row relating to Diesel particulate matter (as respirable elemental carbon) by — 
	(a)	deleting the 8‑hour time weighted average (TWA) of 0.01 mg/m3; and
	(b)	inserting the 8‑hour time weighted average (TWA) of 0.1 mg/m3 (measured as sub‑micron elemental carbon).
	(3)	The Table in Appendix A is modified in the row relating to Phosphine by deleting the 8‑hour time weighted averages (TWA) of 0.05 ppm and 0.07 mg/m3 and the peak limits of 0.15 ppm and 0.21 mg/m3 and inserting the following exposure limits — 
	(a)	8‑hour time weighted average (TWA) — 
	(i)	0.3 ppm; and
	(ii)	0.42 mg/m3;
	(b)	short term exposure limit (STEL) — 
	(i)	1 ppm; and
	(ii)	1.4 mg/m3.
	(4)	In this regulation, each of the following terms has the same meaning as in the Workplace exposure limits for airborne contaminants — 
	8‑hour time weighted average (TWA)
	peak limitation (peak limit)
	short term exposure limit (STEL)
	(5)	The modification in subregulation (3) applies until 30 November 2029.

[bookmark: _Toc244776091][bookmark: _Toc244776737]21.	Regulation 49 amended
	(1)	In regulation 49(1) delete “standard” and insert:

		limit

	(2)	In regulation 49(2):
	(a)	delete “standard” and insert:

		limit

	(b)	delete “time‑weighted” and insert:

		time weighted

	(c)	in paragraph (a) delete “mg per cubic metre of air;” and insert:

		mg/m3;

	(d)	in paragraph (b) delete “mg per cubic metre of air.” and insert:

		mg/m3.

	(3)	In regulation 49(3):
	(a)	delete “Workplace Exposure Standards for Airborne Contaminants” and insert:

		Workplace exposure limits for airborne contaminants

	(b)	delete “standard referred to in those Standards.” and insert:

		limit referred to in that document.

	(4)	Delete regulation 49(4) and insert:

	(4)	In subregulation (2), each of the following terms has the same meaning as in the Workplace exposure limits for airborne contaminants — 
	8‑hour time weighted average
	inhalable
	respirable

	Note: The heading to amended regulation 49 is to read:
		Ensuring exposure limits for substances and mixtures not exceeded
[bookmark: _Toc244776092][bookmark: _Toc244776738]22.	Regulation 50 amended
		In regulation 50(1):
	(a)	delete “standard” (1st occurrence) and insert:

		limit

	(b)	in paragraph (a) delete “standard; or” and insert:

		limit; or

[bookmark: _Toc244776093][bookmark: _Toc244776739]23.	Regulation 352 amended
		In regulation 352(c) delete “standard;” and insert:

		limit;

[bookmark: _Toc244776094][bookmark: _Toc244776740]24.	Regulation 420 amended
		In regulation 420(2) delete “standard” and insert:

		limit

[bookmark: _Toc244776095][bookmark: _Toc244776741]25.	Regulation 454 amended
		In regulation 454(2)(a) delete “to below the exposure standard; and” and insert:

		below the exposure limit for asbestos; and

[bookmark: _Toc244776096][bookmark: _Toc244776742]26.	Regulation 455 amended
		In regulation 455(2) delete “to below the exposure standard.” and insert:

		below the exposure limit for asbestos.

[bookmark: _Toc244776097][bookmark: _Toc244776743]27.	Regulation 482 amended
		In regulation 482(1) and (2) delete “standard” and insert:

		limit for asbestos

[bookmark: _Toc244776098][bookmark: _Toc244776744]28.	Regulation 637 amended
		In regulation 637(1)(b)(i) and (ii) delete “standard” and insert:

		limit

[bookmark: _Toc244776099][bookmark: _Toc244776745]29.	Regulation 637A amended
	(1)	In regulation 637A(1) and (2) delete “standard” and insert:

		limit

	(2)	In regulation 637A(3)(a) delete “standard” and insert:

		limit

	Note: The heading to amended regulation 637A is to read:
		Requirements if airborne exposure limit for mixture or substance exceeded
[bookmark: _Toc244776100][bookmark: _Toc244776746]30.	Regulation 648 amended
		In regulation 648(1):
	(a)	in paragraph (b)(ii) delete “49;” and insert:

		49.

	(b)	after paragraph (b) delete “and”;
	(c)	delete paragraph (c).
[bookmark: _Toc244776101][bookmark: _Toc244776747]31.	Regulation 650 amended
		In regulation 650(1):
	(a)	in paragraph (b) delete “exceeded; or” and insert:

		exceeded.

	(b)	delete paragraph (c).
	Note: The heading to amended regulation 650 is to read:
		Requirements if air quality requirements or exposure limits not complied with
[bookmark: _Toc244776102][bookmark: _Toc244776748]32.	Regulation 656B deleted
		Delete regulation 656B.
[bookmark: _Toc244776103][bookmark: _Toc244776749]33.	Schedule 8 amended
		In Schedule 8 clause 3(2)(a)(iv) delete “standard” and insert:

		limit
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