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Road Traffic (Vehicles) Act 2012
Road Traffic (Vehicles) Amendment Regulations (No. 3) 2024
Made by the Governor in Executive Council.
[bookmark: _Toc175825418][bookmark: _Toc176252789]1.	Citation
[bookmark: Start_Cursor]		These regulations are the Road Traffic (Vehicles) Amendment Regulations (No. 3) 2024.
[bookmark: _Toc175825419][bookmark: _Toc176252790]2.	Commencement
		These regulations come into operation as follows —
	(a)	regulations 1 and 2 — on the day on which these regulations are published on the WA legislation website;
	(b)	the rest of the regulations — on the day after that day.
[bookmark: _Toc175825420][bookmark: _Toc176252791]3.	Regulations amended
		These regulations amend the Road Traffic (Vehicles) Regulations 2014.
[bookmark: _Toc175825421][bookmark: _Toc176252792]4.	Regulation 171 amended
		Delete regulation 171(1) and insert:

	(1A)	In this regulation — 
	safer freight vehicle means a heavy vehicle, other than a trailer or bus, that — 
	(a)	meets the requirements of the following ADRs, so far as they are applicable — 
	(i)	ADR 14/03 or a later version of ADR 14;
	(ii)	ADR 35/07 or a later version of ADR 35;
	(iii)	ADR 97;
	(iv)	ADR 99;
		and
	(b)	if the vehicle has a GVM of more than 8 t — meets the requirements of ADR 105, so far as it is applicable; and
	(c)	if the vehicle is not a prime mover — 
	(i)	meets the requirements of ADR 106; and
	(ii)	is fitted with conspicuity markings that comply with the requirements of ADR 13.
	(1)	A motor vehicle, trailer or any vehicle in a combination must not be over — 
	(a)	if the vehicle is a safer freight vehicle — 2.55 m wide; or
	(b)	otherwise — 2.5 m wide.
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		In regulation 180(2) delete:

Vehicle loaded to width limits mentioned in r. 170, 
with maximum side projection of load allowed under r. 180

		and insert:

Maximum width limit of vehicle and its load set under r. 171(1)(b), with maximum side projection of load allowed under r. 180
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