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Road Traffic (Vehicles) Act 2012
Road Traffic (Vehicles) Amendment Regulations (No. 4) 2025
Made by the Governor in Executive Council.
[bookmark: _Toc208493337][bookmark: _Toc208915168]1.	Citation
[bookmark: Start_Cursor]		These regulations are the Road Traffic (Vehicles) Amendment Regulations (No. 4) 2025.
[bookmark: _Toc208493338][bookmark: _Toc208915169]2.	Commencement
		These regulations come into operation as follows —
	(a)	regulations 1 and 2 — on the day on which these regulations are published on the WA legislation website;
	(b)	the rest of the regulations — on 1 January 2026.
[bookmark: _Toc208493339][bookmark: _Toc208915170]3.	Regulations amended
		These regulations amend the Road Traffic (Vehicles) Regulations 2014.
[bookmark: _Toc208493340][bookmark: _Toc208915171]4.	Regulation 8 amended
		Delete regulation 8(2) and insert:

	(2)	If a diagram is referred to in a provision, the diagram has effect in accordance with the provision.
	Note for this subregulation:
		See regulations 362B(4)(d), 362C(4)(d) and 373(3)(a).
	(3)	A diagram is otherwise for illustrative purposes only and is not intended to represent the actual size, dimensions or colour of the thing shown.

[bookmark: _Toc208493341][bookmark: _Toc208915172]5.	Regulation 117 amended
		In regulation 117(1) delete “127, 133 and 362(2),” and insert:

		127 and 133,

[bookmark: _Toc208493342][bookmark: _Toc208915173]6.	Regulation 121 amended
		In regulation 121(b) delete “362(2).” and insert:

		136, 362(2) or (3), 362B or 362C.

[bookmark: _Toc208493343][bookmark: _Toc208915174]7.	Part 10 Divisions 11A and 11B inserted
		After Part 10 Division 11 insert:

[bookmark: _Toc208493344][bookmark: _Toc208493459][bookmark: _Toc208493513][bookmark: _Toc208493647][bookmark: _Toc208914481][bookmark: _Toc208915175]Division 11A — Hydrogen-powered vehicles
[bookmark: _Toc208493345][bookmark: _Toc208915176]362B.	Label requirements for hydrogen‑powered vehicles
	(1)	In this regulation — 
	hydrogen‑powered vehicle means a vehicle that — 
	(a)	is powered by a hydrogen fuel system; and
	(b)	has 1 or more hydrogen fuel containers fitted to the vehicle for the system.
	(2)	This regulation applies to a hydrogen‑powered vehicle — 
	(a)	built on or after 1 January 2019; or
	(b)	modified to be a hydrogen‑powered vehicle on or after 1 January 2019.
	(3)	The vehicle must have fixed conspicuously to its front and rear number plates — 
	(a)	for a vehicle fitted with 1 hydrogen fuel container — a label that complies with subregulation (4); or
	(b)	for a vehicle fitted with 2 or more hydrogen fuel containers — 2 labels that comply with subregulation (4).
	(4)	For the purposes of subregulation (3), a label complies with this subregulation if — 
	(a)	it is affixed to a plate made of metal that is at least 1 mm thick; and
	(b)	the label, and the plate to which it is affixed, is a regular pentagonal shape — 
	(i)	each side of which is 20 mm long; and
	(ii)	each interior angle of which is 108°;
		and
	(c)	it has a yellow surface that complies with class 2 of AS 1906.1:2017 Retroreflective materials and devices for road traffic control purposes — Retroreflective sheeting; and
	(d)	it is marked ‘H’ in a black capital letter that is at least 10 mm high and has the orientation shown in the diagram below; and
	(e)	it is fixed to the number plates so that the letter on the label is in an upright position; and
	(f)	it does not wholly or partly obscure any characters on the number plates.
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Hydrogen‑powered vehicle label
[bookmark: _Toc208493346][bookmark: _Toc208493461][bookmark: _Toc208493515][bookmark: _Toc208493649][bookmark: _Toc208914483][bookmark: _Toc208915177]Division 11B — Electric‑powered vehicles
[bookmark: _Toc208493347][bookmark: _Toc208915178]362C.	Label requirements for electric‑powered vehicles
	(1)	In this regulation — 
	electric‑powered vehicle means a vehicle that is powered by 1 or more electric motors or traction motors that — 
	(a)	are the only propulsion system for the vehicle; or
	(b)	are used in conjunction with another propulsion system for the vehicle.
	(2)	This regulation — 
	(a)	applies to an electric‑powered vehicle — 
	(i)	built on or after 1 January 2019; or
	(ii)	modified to be an electric‑powered vehicle on or after 1 January 2019;
		but
	(b)	does not apply to a vehicle to which regulation 362B applies (even if the vehicle is fitted with an electric motor or traction motor that is used in conjunction with a hydrogen fuel system for the propulsion of the vehicle).
	(3)	The vehicle must have fixed conspicuously to its front and rear number plates a label that complies with subregulation (4).
	(4)	For the purposes of subregulation (3), a label complies with this subregulation if — 
	(a)	it is affixed to a plate made of metal that is at least 1 mm thick; and
	(b)	the label, and the plate to which it is affixed, is an equilateral triangular shape — 
	(i)	each side of which is 30 mm long; and
	(ii)	each interior angle of which is 60°;
		and
	(c)	it has a blue surface that complies with class 2 of AS 1906.1:2017 Retroreflective materials and devices for road traffic control purposes — Retroreflective sheeting; and
	(d)	it is marked ‘EV’ in white capital letters that are at least 8 mm high and have the orientation shown in the diagram below; and
	(e)	it is fixed to the number plates so that the letters on the label are in an upright position; and
	(f)	it does not wholly or partly obscure any characters on the number plates.
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Electric‑powered vehicle label
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